Jacob Wakefield

Assignment 2 Part 2

CSC565

11/11/2018



S1 – 146.7.45.64/25

S2 – 146.7.45.128/24

S3 – 146.7.45.16/27

1. There would not be duplicate mac address in the ARP tables of the router. Each network interface card has a unique mac address.